**Rules:**

**Farm Stock, Non Turbo and Turbo**

-All General Rules Apply

-Stock Block or OEM Replacement

-Stock Appearing fuel system

-Turbo Classes-

Add-on/Aftermarket Turbos allowed but must utilize OEM/M&W maniolds

-Must have working PTO/Belt Pulley and/or Hydraulics

-No Cut Tires

-Factory Side shields allowed, no custom made

-Front Wheel Assist and/or Duals allowed (Still have to make Weight)

-No Aluminum replacement parts

**After Chores**

-All General Rules Apply

-Factory Engine & Drivetrain for Model of tractor

-Fenders Required

-Any Cut Tire Allowed,

-No RPM Limit

-Factory Appearing Fuel System:

Gas-No Downdraft Carburetors(JD 2-Cylinder may upgrade to Duplex).

 Diesel-Factory Type Injection Pump

-No Water Injection

-Factory Appearing Turbocharger

**Altered Farm**

-All General Rules Apply

-2.6 Turbo Limit

-Factory Intake and Exhaust

-20.8x42 Tire Limit, no Aluminum Rear Wheels

-No Water Injection

-Stock Body Injection Pump

-Fuel Dump valve and Air Shutoff

-Steel Flywheel

-Wheelie bars

**Improved Farm**

-All General Rules Apply

-2.8 Turbo Limit

-Stock Appearing Injection Pump

-Required Safety Equipment

 Steel Flywheel, Wheelie Bars, Roll Bar or Cage, Scatter Blanket

 Fuel Dump Valve and Air Shutoff

-20.8-38 Max Tire Size