2026 Polk County Fair Tractor Pull
General Rules
Be a professional, tractors must operate in a safe manner at all times. No chain jerking or hot-rodding on the grounds allowed.  
A driver’s meeting will be held prior to event start time. 

Pullers must be 18 years of age or older to participate. Minors must have parent or guardian consent. No on under the age of 18 will pull outside the Farm Stock Classes. No one younger than 12 years of age will be allowed to pull. 
-Hook Point height MAXIMUM will be 20 inches. Hook point WILL BE UNOBSTRUCTED.
-All pulls must start with a tight chain
-All pullers or a 3”Wide x 3.75”Long Opening 
-Use of a Clevis or Hooking through a Hammer Strap will not be permitted. 
-2 Hook Limit
-Pulling order will be determined by random draw. All pullers must pull in assigned order within three minutes or be subject to disqualification. 
-No going over the Speed Limit, going over will result in a Disqualification, however you may finish your pull.
-Operator must remain seated and drive in a safe manner. 
-All tractors must be in neutral or park when being hooked or unhooked from sled. “Hands up” signal by the driver will be used to indicate this is being followed.  
-Tractor must remain within the boundaries of the track, drivers will obey the flagman.     Failure to do so may result in disqualification. 
-Loss of any weight or part of the tractor while green flag is displayed, will be grounds for disqualification. 
-Tractors will be stopped if front wheels are more than 24” off the ground.  
-Contestants will have two consecutive attempts and 100 feet to start the sled. 
-No First Puller Re-hook
-Class pulling order and drivers order will be posted. 
-Judges have the option to reposition any puller in a class and adjust class running order based on class participation.  
-All tractors must scale prior to hooking to sled, immediately prior to the start of your class.
-100lbs Grace Weight for all classes
-Once weighed, you are staged. Leaving the staging area is not allowed.  
-No Jumping Classes, Tractors that run in a Farm Stock Class cannot go up, Tractors that run Ater Chores or Higher may Not run in Farm Stock.
-NO BEER OR ALCOHOL IN PIT!!! No consumption of alcohol until all pulling by contestant is completed.  
-Failure to obey track officials may result in disqualification and may lead to removal from event.

-Track officials have the right to move a puller to a different class. Additionally, they reserve the right to remove tractors without the required safety equipment from a class.



Classes & Payout
Note: Payouts for 1st, 2nd, and 3rd. 


Farm Stock Non Turbo- $100, $75, $50
7500        -6 MPH
9500        -6 MPH
10500       -6 MPH


Farm Stock Turbo- $100, $75, $50
7500         -8 MPH
8500         -8 MPH
9500         -8 MPH
11000       -12 MPH
13000       -12 MPH
15000       -12 MPH
18000       -12 MPH

After Chores- $150, $100, $60
4500
5500
6500
7500
10500
12500
14500
16500

Altered Farm- $175, $125, $75
11000
12000

Pro Farm- $300, $200, $100
9000
9500

Modified/Open- $300, $200, $100
6500
9300








Rules:
Farm Stock, Non Turbo and Turbo
-All General Rules Apply
-Stock Block or OEM Replacement
-Stock Appearing fuel system
-Turbo Classes-
Add-on/Aftermarket Turbos allowed but must utilize OEM/M&W maniolds
-Must have working PTO/Belt Pulley and/or Hydraulics
-No Full Cut Tires
-Factory Side shields allowed, no custom made
-Front Wheel Assist and/or Duals allowed (Still have to make Weight)
-No Aluminum replacement covers

After Chores
-All General Rules Apply
-Factory Engine & Drivetrain for Model of tractor
-Fenders Recommended
-Any Cut Tire Allowed
-2.4 Turbo Limit, No RPM Limit
-Factory Appearing Fuel System: 
Gas-No Downdraft Carburetors(JD 2-Cylinder may upgrade to Duplex). 
	Diesel-Factory Type Injection Pump

Altered Farm
-All General Rules Apply
-2.6 Turbo Limit
-Factory Intake and Exhaust
-20.8x42 Tire Limit, no Aluminum Rear Wheels
-No Water Injection
-Stock Body Injection Pump
-Fuel Dump valve and Air Shutoff Steel Flywheel & Wheelie bars

Pro Farm
-All General Rules Apply
-Required Safety Equipment
	Steel Flywheel, Wheelie Bars, Roll Cage, Scatter Blanket
	Fuel Dump Valve and Air Shutoff
	Helment and Firesuit
-466 Cubic Inch Limit
-3x3 Turbo
-Any Injection Pump
-Water Injection Allowed
-20.8 x 38 Max Tire, Any Cut

Modifed/Open
-All General Rules Apply
-Required Safety Equipment
	Steel Flywheel, Wheelie Bars, Roll Cage, Scatter Blanket
	Fuel Dump Valve and Air Shutoff
	Helment and Firesuit

Class Order
Note: Line up Subject to Change
 
4500 After Chore
5500 After Chore 
7500 Farm Stock Non Turbo 6 MPH 
6500 After Chore
7500 Farm Stock Turbo 8 MPH  
6500 Modified/Open
7500 After Chore
8500 Farm Stock Turbo 8 MPH
9500 Farm Stock Non Turbo 6 MPH 
9500 Farm Stock Turbo 8 MPH 
9000 Pro Farm
10500 Farm Stock Non Turbo 6 MPH
10500 After Chore 
11000 Altered Farm 2.6
9300 Open
11000 Farm Stock Turbo 12 MPH 
12000 Altered Farm 2.6
12500 After Chore 
9500 Pro Farm
13000 Farm Stock Turbo 12 MPH 
14500 After Chore
15000 Farm Stock Turbo 12 MPH 
16500 After Chore
18000 Farm Stock Turbo 12MPH
