2026 Polk County Fair Sunday Pull
General Rules
Be a professional, tractors must operate in a safe manner at all times. No chain jerking or hot-rodding on the grounds allowed.  
A driver’s meeting will be held prior to event start time. 

Pullers must be 18 years of age or older to participate. Minors must have parent or guardian consent. No on under the age of 18 will pull outside the Farm Stock Classes. No one younger than 12 years of age will be allowed to pull. 
-Hook Point height MAXIMUM will be 20 inches. Hook point WILL BE UNOBSTRUCTED.
-All pulls must start with a tight chain
-All pullers or a 3”Wide x 3.75”Long Opening 
-Use of a Clevis or Hooking through a Hammer Strap will not be permitted. 
-2 Hook Limit 
-Pulling order will be determined by random draw. All pullers must pull in assigned order within three minutes or be subject to disqualification. 
-No going over the Speed Limit, going over will result in a Disqualification, however you may finish your pull.
-Operator must remain seated and drive in a safe manner. 
-All tractors must be in neutral or park when being hooked or unhooked from sled. “Hands up” signal by the driver will be used to indicate this is being followed.  
-Tractor must remain within the boundaries of the track, drivers will obey the flagman.     Failure to do so may result in disqualification. 
-Loss of any weight or part of the tractor will be grounds for disqualification. 
-Tractors will be stopped if front wheels are more than 24” off the ground.  
-Contestants will have two consecutive attempts and 100 feet to start the sled. 
-No First Puller Re-hook
-Class pulling order and drivers order will be posted. 
-Judges have the option to reposition any puller in a class and adjust class running order based on class participation.  
-All tractors must scale prior to hooking to sled, immediately prior to the start of your class.
-100lbs Grace Weight for all classes
-Once weighed, you are staged. Leaving the staging area is not allowed.  
-No Jumping Classes, Tractors will run 4 Mph or 7 Mph, not both.
-NO BEER OR ALCOHOL IN PIT!!! No consumption of alcohol until all pulling by contestant is completed.  
-Failure to obey track officials may result in disqualification and may lead to removal from event.

-Track officials have the right to move a puller to a different class. Additionally, they reserve the right to remove tractors without the required safety equipment from a class.



Classes & Payout
4 Mph Classic 1959 & Older- $100, $75, $50
4000
4500
5500
6500
7500
9000

7 Mph Improved 1959 & Older- $100, $75, $50
4100
4600
5600
6600

Class Order
4000 4mph
4100 7mph
4500 4mph
4600 7mph
5500 4mph
5600 7mph
6500 4mph
6600 7mph
7500 4mph
9000 4mph

4 Mph Classic 1959 & Older
-All General Rules Apply
-Tractors should appear as close to factory as possible. No stripping parts or Aluminum replacement parts.
-Fenders Recommended
-Must have PTO or Hydraulics, or Factory Block Offs, no custom made cover plates.
-Engines will have working govenors, Cast iron Manifolds, Factory Carbuerators/Injection Pump with Factory Air Cleaner
-No Cut Tires, No pressed Steel Rims. 15.5-38 Max for 4000 & 4500, 18.4-38 Max for 5500 & 6500

7 Mph Improved 1959 & Older
-All General Rules Apply
-Factory or Ag Based Replacement Engine matching the OEM Drivetrain
-Fenders Recommended
-Any Cut Tire Allowed, 18.4-38 Max Size
-No RPM Limit
-Factory Appearing Fuel System: 
Gas-No Downdraft Carburetors(JD 2-Cylinder may upgrade to Duplex). 
	Diesel-Factory Type Injection Pump
-Headers Allowed 

